5.15Hz for Theta = 5 degrees

time = 36.3 us

high k gives us chatter/vibration due to saturating after one encoder count or .09 degrees

Our optimal value was 650, no chatter, but strong wall